(module Motor_Connector (layer F.Cu) (tedit 5F0A0813)
  (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Motor_Connector (at 0 -0.5) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user REF** (at 0 0.5 180) (layer B.SilkS) hide
    (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
  )
  (fp_text user Motor_Connector (at -17.9 0) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (pad 2 smd rect (at 0 0) (size 3 5.4) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at 0 8.2) (size 3 5.4) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at 0 -8.2) (size 3 5.4) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at 0 -8.2 180) (size 3 5.4) (layers B.Cu B.Paste B.Mask))
  (pad 1 smd rect (at 0 8.2 180) (size 3 5.4) (layers B.Cu B.Paste B.Mask))
  (pad 2 smd rect (at 0 0 180) (size 3 5.4) (layers B.Cu B.Paste B.Mask))
)
