(module Lattice_QFN-48UP (layer F.Cu) (tedit 5DE35271)
  (fp_text reference REF** (at 0 0) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value %V (at 0 -0.5) (layer F.Fab) hide
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user %R (at 0 0) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -3.7 -3.07) (end -3.07 -3.7) (layer F.SilkS) (width 0.15))
  (fp_line (start -3.7 3.7) (end -3.7 3.07) (layer F.SilkS) (width 0.15))
  (fp_line (start -3.07 3.7) (end -3.7 3.7) (layer F.SilkS) (width 0.15))
  (fp_line (start 3.07 3.7) (end 3.7 3.7) (layer F.SilkS) (width 0.15))
  (fp_line (start 3.7 3.7) (end 3.7 3.07) (layer F.SilkS) (width 0.15))
  (fp_line (start 3.7 -3.07) (end 3.7 -3.7) (layer F.SilkS) (width 0.15))
  (fp_line (start 3.7 -3.7) (end 3.07 -3.7) (layer F.SilkS) (width 0.15))
  (fp_circle (center -3.7 -3.7) (end -3.7 -3.85) (layer F.SilkS) (width 0.15))
  (fp_line (start -3.25 -3.55) (end -3.55 -3.25) (layer F.Fab) (width 0.15))
  (fp_line (start 3.55 -3.55) (end -3.25 -3.55) (layer F.Fab) (width 0.15))
  (fp_line (start 3.55 3.55) (end 3.55 -3.55) (layer F.Fab) (width 0.15))
  (fp_line (start -3.55 3.55) (end 3.55 3.55) (layer F.Fab) (width 0.15))
  (fp_line (start -3.55 -3.25) (end -3.55 3.55) (layer F.Fab) (width 0.15))
  (fp_line (start -3.8 -3.02) (end -3.8 -3.8) (layer F.CrtYd) (width 0.15))
  (fp_line (start -3.8 -3.8) (end 3.8 -3.8) (layer F.CrtYd) (width 0.15))
  (fp_line (start 3.8 -3.8) (end 3.8 -3.02) (layer F.CrtYd) (width 0.15))
  (fp_line (start 3.8 -3.02) (end 4.05 -3.02) (layer F.CrtYd) (width 0.15))
  (fp_line (start 4.05 -3.02) (end 4.05 3.02) (layer F.CrtYd) (width 0.15))
  (fp_line (start 4.05 3.02) (end 3.8 3.02) (layer F.CrtYd) (width 0.15))
  (fp_line (start 3.8 3.02) (end 3.8 3.8) (layer F.CrtYd) (width 0.15))
  (fp_line (start 3.8 3.8) (end -3.8 3.8) (layer F.CrtYd) (width 0.15))
  (fp_line (start -3.8 3.8) (end -3.8 3.02) (layer F.CrtYd) (width 0.15))
  (fp_line (start -3.8 3.02) (end -4.05 3.02) (layer F.CrtYd) (width 0.15))
  (fp_line (start -4.05 3.02) (end -4.05 -3.02) (layer F.CrtYd) (width 0.15))
  (fp_line (start -4.05 -3.02) (end -3.8 -3.02) (layer F.CrtYd) (width 0.15))
  (pad 1 smd roundrect (at -3.5 -2.75) (size 0.8 0.24) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
    (solder_mask_margin 0.07))
  (pad 2 smd roundrect (at -3.5 -2.25) (size 0.8 0.24) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
    (solder_mask_margin 0.07))
  (pad 3 smd roundrect (at -3.5 -1.75) (size 0.8 0.24) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
    (solder_mask_margin 0.07))
  (pad 4 smd roundrect (at -3.5 -1.25) (size 0.8 0.24) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
    (solder_mask_margin 0.07))
  (pad 5 smd roundrect (at -3.5 -0.75) (size 0.8 0.24) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
    (solder_mask_margin 0.07))
  (pad 6 smd roundrect (at -3.5 -0.25) (size 0.8 0.24) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
    (solder_mask_margin 0.07))
  (pad 7 smd roundrect (at -3.5 0.25) (size 0.8 0.24) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
    (solder_mask_margin 0.07))
  (pad 8 smd roundrect (at -3.5 0.75) (size 0.8 0.24) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
    (solder_mask_margin 0.07))
  (pad 9 smd roundrect (at -3.5 1.25) (size 0.8 0.24) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
    (solder_mask_margin 0.07))
  (pad 10 smd roundrect (at -3.5 1.75) (size 0.8 0.24) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
    (solder_mask_margin 0.07))
  (pad 11 smd roundrect (at -3.5 2.25) (size 0.8 0.24) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
    (solder_mask_margin 0.07))
  (pad 12 smd roundrect (at -3.5 2.75) (size 0.8 0.24) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
    (solder_mask_margin 0.07))
  (pad 13 smd roundrect (at -2.75 3.5) (size 0.24 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
    (solder_mask_margin 0.07))
  (pad 14 smd roundrect (at -2.25 3.5) (size 0.24 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
    (solder_mask_margin 0.07))
  (pad 15 smd roundrect (at -1.75 3.5) (size 0.24 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
    (solder_mask_margin 0.07))
  (pad 16 smd roundrect (at -1.25 3.5) (size 0.24 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
    (solder_mask_margin 0.07))
  (pad 17 smd roundrect (at -0.75 3.5) (size 0.24 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
    (solder_mask_margin 0.07))
  (pad 18 smd roundrect (at -0.25 3.5) (size 0.24 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
    (solder_mask_margin 0.07))
  (pad 19 smd roundrect (at 0.25 3.5) (size 0.24 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
    (solder_mask_margin 0.07))
  (pad 20 smd roundrect (at 0.75 3.5) (size 0.24 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
    (solder_mask_margin 0.07))
  (pad 21 smd roundrect (at 1.25 3.5) (size 0.24 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
    (solder_mask_margin 0.07))
  (pad 22 smd roundrect (at 1.75 3.5) (size 0.24 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
    (solder_mask_margin 0.07))
  (pad 23 smd roundrect (at 2.25 3.5) (size 0.24 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
    (solder_mask_margin 0.07))
  (pad 24 smd roundrect (at 2.75 3.5) (size 0.24 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
    (solder_mask_margin 0.07))
  (pad 25 smd roundrect (at 3.5 2.75) (size 0.8 0.24) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
    (solder_mask_margin 0.07))
  (pad 26 smd roundrect (at 3.5 2.25) (size 0.8 0.24) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
    (solder_mask_margin 0.07))
  (pad 27 smd roundrect (at 3.5 1.75) (size 0.8 0.24) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
    (solder_mask_margin 0.07))
  (pad 28 smd roundrect (at 3.5 1.25) (size 0.8 0.24) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
    (solder_mask_margin 0.07))
  (pad 29 smd roundrect (at 3.5 0.75) (size 0.8 0.24) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
    (solder_mask_margin 0.07))
  (pad 30 smd roundrect (at 3.5 0.25) (size 0.8 0.24) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
    (solder_mask_margin 0.07))
  (pad 31 smd roundrect (at 3.5 -0.25) (size 0.8 0.24) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
    (solder_mask_margin 0.07))
  (pad 32 smd roundrect (at 3.5 -0.75) (size 0.8 0.24) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
    (solder_mask_margin 0.07))
  (pad 33 smd roundrect (at 3.5 -1.25) (size 0.8 0.24) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
    (solder_mask_margin 0.07))
  (pad 34 smd roundrect (at 3.5 -1.75) (size 0.8 0.24) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
    (solder_mask_margin 0.07))
  (pad 35 smd roundrect (at 3.5 -2.25) (size 0.8 0.24) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
    (solder_mask_margin 0.07))
  (pad 36 smd roundrect (at 3.5 -2.75) (size 0.8 0.24) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
    (solder_mask_margin 0.07))
  (pad 37 smd roundrect (at 2.75 -3.5) (size 0.24 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
    (solder_mask_margin 0.07))
  (pad 38 smd roundrect (at 2.25 -3.5) (size 0.24 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
    (solder_mask_margin 0.07))
  (pad 39 smd roundrect (at 1.75 -3.5) (size 0.24 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
    (solder_mask_margin 0.07))
  (pad 40 smd roundrect (at 1.25 -3.5) (size 0.24 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
    (solder_mask_margin 0.07))
  (pad 41 smd roundrect (at 0.75 -3.5) (size 0.24 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
    (solder_mask_margin 0.07))
  (pad 42 smd roundrect (at 0.25 -3.5) (size 0.24 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
    (solder_mask_margin 0.07))
  (pad 43 smd roundrect (at -0.25 -3.5) (size 0.24 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
    (solder_mask_margin 0.07))
  (pad 44 smd roundrect (at -0.75 -3.5) (size 0.24 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
    (solder_mask_margin 0.07))
  (pad 45 smd roundrect (at -1.25 -3.5) (size 0.24 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
    (solder_mask_margin 0.07))
  (pad 46 smd roundrect (at -1.75 -3.5) (size 0.24 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
    (solder_mask_margin 0.07))
  (pad 47 smd roundrect (at -2.25 -3.5) (size 0.24 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
    (solder_mask_margin 0.07))
  (pad 48 smd roundrect (at -2.75 -3.5) (size 0.24 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
    (solder_mask_margin 0.07))
  (pad 0 smd rect (at 0 0) (size 5.5 5.5) (layers F.Cu F.Mask) (solder_mask_margin 0.07))
  (fp_poly (pts (xy 0.1499999999999999 -2.65) (xy 0.1499999999999999 -0.1499999999999999) (xy 2.65 -0.1499999999999999) (xy 2.65 -2.65)) (layer F.Paste)  (width 0.1))
  (fp_poly (pts (xy -2.65 -2.65) (xy -2.65 -0.1499999999999999) (xy -0.1499999999999999 -0.1499999999999999) (xy -0.1499999999999999 -2.65)) (layer F.Paste)  (width 0.1))
  (fp_poly (pts (xy -2.65 0.1499999999999999) (xy -2.65 2.65) (xy -0.1499999999999999 2.65) (xy -0.1499999999999999 0.1499999999999999)) (layer F.Paste)  (width 0.1))
  (fp_poly (pts (xy 0.1499999999999999 0.1499999999999999) (xy 0.1499999999999999 2.65) (xy 2.65 2.65) (xy 2.65 0.1499999999999999)) (layer F.Paste)  (width 0.1))
)
