(module R_2512_6332Metric_Sense (layer F.Cu) (tedit 6069ACE8)
  (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
  (tags resistor)
  (attr smd)
  (fp_text reference REF** (at -0.01 -2.89) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value R_2512_6332Metric_Sense (at 0 2.62) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -3.15 1.6) (end -3.15 -1.6) (layer F.Fab) (width 0.1))
  (fp_line (start -3.15 -1.6) (end 3.15 -1.6) (layer F.Fab) (width 0.1))
  (fp_line (start 3.15 -1.6) (end 3.15 1.6) (layer F.Fab) (width 0.1))
  (fp_line (start 3.15 1.6) (end -3.15 1.6) (layer F.Fab) (width 0.1))
  (fp_line (start -2.177064 -2.1) (end 2.177064 -2.1) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.177064 2.1) (end 2.177064 2.1) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.82 1.92) (end -3.82 -1.92) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.82 -1.92) (end 3.82 -1.92) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3.82 -1.92) (end 3.82 1.92) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3.82 1.92) (end -3.82 1.92) (layer F.CrtYd) (width 0.05))
  (fp_text user %R (at 0 0) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (pad 2 smd roundrect (at -2.5 0) (size 3.4 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.164))
  (pad 1 smd roundrect (at -2.5 -1.4) (size 3.4 1.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.164))
  (pad 1 smd roundrect (at -2.5 1.4) (size 3.4 1.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.164))
  (pad 3 smd roundrect (at 2.5 0) (size 3.4 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.164))
  (pad 4 smd roundrect (at 2.5 1.4) (size 3.4 1.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.164))
  (pad 4 smd roundrect (at 2.5 -1.4) (size 3.4 1.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.164))
  (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
