{
  "board": {
    "3dviewports": [],
    "design_settings": {
      "defaults": {
        "apply_defaults_to_fp_fields": false,
        "apply_defaults_to_fp_shapes": false,
        "apply_defaults_to_fp_text": false,
        "board_outline_line_width": 0.05,
        "copper_line_width": 0.2,
        "copper_text_italic": false,
        "copper_text_size_h": 1.5,
        "copper_text_size_v": 1.5,
        "copper_text_thickness": 0.3,
        "copper_text_upright": false,
        "courtyard_line_width": 0.05,
        "dimension_precision": 1,
        "dimension_units": 0,
        "dimensions": {
          "arrow_length": 1270000,
          "extension_offset": 500000,
          "keep_text_aligned": true,
          "suppress_zeroes": false,
          "text_position": 0,
          "units_format": 1
        },
        "fab_line_width": 0.1,
        "fab_text_italic": false,
        "fab_text_size_h": 1.0,
        "fab_text_size_v": 1.0,
        "fab_text_thickness": 0.15,
        "fab_text_upright": false,
        "other_line_width": 0.1,
        "other_text_italic": false,
        "other_text_size_h": 1.0,
        "other_text_size_v": 1.0,
        "other_text_thickness": 0.15,
        "other_text_upright": false,
        "pads": {
          "drill": 0.762,
          "height": 1.524,
          "width": 1.524
        },
        "silk_line_width": 0.12,
        "silk_text_italic": false,
        "silk_text_size_h": 1.0,
        "silk_text_size_v": 1.0,
        "silk_text_thickness": 0.15,
        "silk_text_upright": false,
        "zones": {
          "45_degree_only": false,
          "min_clearance": 0.508
        }
      },
      "diff_pair_dimensions": [
        {
          "gap": 0.0,
          "via_gap": 0.0,
          "width": 0.0
        },
        {
          "gap": 0.0,
          "via_gap": 0.0,
          "width": 0.0
        },
        {
          "gap": 0.0,
          "via_gap": 0.0,
          "width": 0.0
        }
      ],
      "drc_exclusions": [],
      "meta": {
        "version": 2
      },
      "rule_severities": {
        "annular_width": "error",
        "clearance": "error",
        "connection_width": "warning",
        "copper_edge_clearance": "error",
        "copper_sliver": "warning",
        "courtyards_overlap": "error",
        "diff_pair_gap_out_of_range": "error",
        "diff_pair_uncoupled_length_too_long": "error",
        "drill_out_of_range": "error",
        "duplicate_footprints": "warning",
        "extra_footprint": "warning",
        "footprint": "error",
        "footprint_symbol_mismatch": "warning",
        "footprint_type_mismatch": "error",
        "hole_clearance": "error",
        "hole_near_hole": "error",
        "holes_co_located": "warning",
        "invalid_outline": "error",
        "isolated_copper": "warning",
        "item_on_disabled_layer": "error",
        "items_not_allowed": "error",
        "length_out_of_range": "error",
        "lib_footprint_issues": "warning",
        "lib_footprint_mismatch": "warning",
        "malformed_courtyard": "error",
        "microvia_drill_out_of_range": "error",
        "missing_courtyard": "ignore",
        "missing_footprint": "warning",
        "net_conflict": "warning",
        "npth_inside_courtyard": "ignore",
        "padstack": "error",
        "pth_inside_courtyard": "ignore",
        "shorting_items": "error",
        "silk_edge_clearance": "warning",
        "silk_over_copper": "ignore",
        "silk_overlap": "ignore",
        "skew_out_of_range": "error",
        "solder_mask_bridge": "error",
        "starved_thermal": "error",
        "text_height": "warning",
        "text_thickness": "warning",
        "through_hole_pad_without_hole": "error",
        "too_many_vias": "error",
        "track_dangling": "warning",
        "track_width": "error",
        "tracks_crossing": "error",
        "unconnected_items": "error",
        "unresolved_variable": "error",
        "via_dangling": "warning",
        "zone_has_empty_net": "error",
        "zones_intersect": "error"
      },
      "rules": {
        "allow_blind_buried_vias": false,
        "allow_microvias": false,
        "max_error": 0.005,
        "min_clearance": 0.1,
        "min_connection": 0.0,
        "min_copper_edge_clearance": 0.2,
        "min_hole_clearance": 0.0,
        "min_hole_to_hole": 0.24,
        "min_microvia_diameter": 0.2,
        "min_microvia_drill": 0.1,
        "min_resolved_spokes": 1,
        "min_silk_clearance": 0.0,
        "min_text_height": 0.8,
        "min_text_thickness": 0.08,
        "min_through_hole_diameter": 0.2,
        "min_track_width": 0.1,
        "min_via_annular_width": 0.05,
        "min_via_annulus": 0.049999999999999996,
        "min_via_diameter": 0.45,
        "solder_mask_to_copper_clearance": 0.0,
        "use_height_for_length_calcs": true
      },
      "teardrop_options": [
        {
          "td_onpadsmd": true,
          "td_onroundshapesonly": false,
          "td_ontrackend": false,
          "td_onviapad": true
        }
      ],
      "teardrop_parameters": [
        {
          "td_allow_use_two_tracks": true,
          "td_curve_segcount": 0,
          "td_height_ratio": 1.0,
          "td_length_ratio": 0.5,
          "td_maxheight": 2.0,
          "td_maxlen": 1.0,
          "td_on_pad_in_zone": false,
          "td_target_name": "td_round_shape",
          "td_width_to_size_filter_ratio": 0.9
        },
        {
          "td_allow_use_two_tracks": true,
          "td_curve_segcount": 0,
          "td_height_ratio": 1.0,
          "td_length_ratio": 0.5,
          "td_maxheight": 2.0,
          "td_maxlen": 1.0,
          "td_on_pad_in_zone": false,
          "td_target_name": "td_rect_shape",
          "td_width_to_size_filter_ratio": 0.9
        },
        {
          "td_allow_use_two_tracks": true,
          "td_curve_segcount": 0,
          "td_height_ratio": 1.0,
          "td_length_ratio": 0.5,
          "td_maxheight": 2.0,
          "td_maxlen": 1.0,
          "td_on_pad_in_zone": false,
          "td_target_name": "td_track_end",
          "td_width_to_size_filter_ratio": 0.9
        }
      ],
      "track_widths": [
        0.0,
        0.127,
        0.13,
        0.147,
        0.2,
        0.23,
        0.5,
        1.0,
        2.0,
        3.0
      ],
      "tuning_pattern_settings": {
        "diff_pair_defaults": {
          "corner_radius_percentage": 80,
          "corner_style": 1,
          "max_amplitude": 1.0,
          "min_amplitude": 0.2,
          "single_sided": false,
          "spacing": 1.0
        },
        "diff_pair_skew_defaults": {
          "corner_radius_percentage": 80,
          "corner_style": 1,
          "max_amplitude": 1.0,
          "min_amplitude": 0.2,
          "single_sided": false,
          "spacing": 0.6
        },
        "single_track_defaults": {
          "corner_radius_percentage": 80,
          "corner_style": 1,
          "max_amplitude": 1.0,
          "min_amplitude": 0.2,
          "single_sided": false,
          "spacing": 0.6
        }
      },
      "via_dimensions": [
        {
          "diameter": 0.0,
          "drill": 0.0
        },
        {
          "diameter": 0.45,
          "drill": 0.25
        }
      ],
      "zones_allow_external_fillets": false,
      "zones_use_no_outline": false
    },
    "ipc2581": {
      "dist": "",
      "distpn": "",
      "internal_id": "",
      "mfg": "",
      "mpn": ""
    },
    "layer_presets": [],
    "viewports": []
  },
  "boards": [],
  "cvpcb": {
    "equivalence_files": []
  },
  "libraries": {
    "pinned_footprint_libs": [],
    "pinned_symbol_libs": []
  },
  "meta": {
    "filename": "breakout.kicad_pro",
    "version": 1
  },
  "net_settings": {
    "classes": [
      {
        "bus_width": 12,
        "clearance": 0.13,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.13,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "Default",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.13,
        "via_diameter": 0.45,
        "via_drill": 0.25,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.13,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.13,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "100R",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.127,
        "via_diameter": 0.45,
        "via_drill": 0.25,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.13,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.178,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "50R",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.13,
        "via_diameter": 0.45,
        "via_drill": 0.25,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.13,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.13,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "75R",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.13,
        "via_diameter": 0.45,
        "via_drill": 0.25,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.13,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.15,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "90R",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.147,
        "via_diameter": 0.45,
        "via_drill": 0.25,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.13,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.13,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "HDMI",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.127,
        "via_diameter": 0.45,
        "via_drill": 0.25,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 1.0,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.13,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "POE TAPS",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.13,
        "via_diameter": 0.45,
        "via_drill": 0.25,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.13,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.13,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "Default",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.13,
        "via_diameter": 0.45,
        "via_drill": 0.25,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.13,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.13,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "100R",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.127,
        "via_diameter": 0.45,
        "via_drill": 0.25,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.13,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.178,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "50R",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.13,
        "via_diameter": 0.45,
        "via_drill": 0.25,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.13,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.13,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "75R",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.13,
        "via_diameter": 0.45,
        "via_drill": 0.25,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.13,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.15,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "90R",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.147,
        "via_diameter": 0.45,
        "via_drill": 0.25,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.13,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.13,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "HDMI",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.127,
        "via_diameter": 0.45,
        "via_drill": 0.25,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 1.0,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.13,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "POE TAPS",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.13,
        "via_diameter": 0.45,
        "via_drill": 0.25,
        "wire_width": 6
      }
    ],
    "meta": {
      "version": 3
    },
    "net_colors": null,
    "netclass_assignments": null,
    "netclass_patterns": [
      {
        "netclass": "Default",
        "pattern": "/+12v"
      },
      {
        "netclass": "Default",
        "pattern": "/RTC , Wakeup, FAN/SDA"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/estop"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/+3V3"
      },
      {
        "netclass": "Default",
        "pattern": "/CM4_GPIO ( Ethernet, GPIO, SDCARD)/GLOBAL_EN"
      },
      {
        "netclass": "Default",
        "pattern": "/CM4_GPIO ( Ethernet, GPIO, SDCARD)/GPIO3"
      },
      {
        "netclass": "Default",
        "pattern": "Net-(D17-A)"
      },
      {
        "netclass": "Default",
        "pattern": "Net-(D20-A)"
      },
      {
        "netclass": "Default",
        "pattern": "/CM4_GPIO ( Ethernet, GPIO, SDCARD)/AIN1"
      },
      {
        "netclass": "Default",
        "pattern": "/CM4_HighSpeed/HDMI0_SDA"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/breakout/+5V_ISO_GND3"
      },
      {
        "netclass": "Default",
        "pattern": "/+3.3v"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/+2V5"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/breakout/d_step_iso"
      },
      {
        "netclass": "Default",
        "pattern": "/CM4_GPIO ( Ethernet, GPIO, SDCARD)/RUN_PG"
      },
      {
        "netclass": "Default",
        "pattern": "unconnected-(U6A-RGB1-Pad40)"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/a_home+"
      },
      {
        "netclass": "Default",
        "pattern": "unconnected-(U3-VC2-Pad12)"
      },
      {
        "netclass": "Default",
        "pattern": "unconnected-(D11-NC-Pad2)"
      },
      {
        "netclass": "Default",
        "pattern": "/CM4_GPIO ( Ethernet, GPIO, SDCARD)/GPIO12"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/fault"
      },
      {
        "netclass": "Default",
        "pattern": "unconnected-(U13-NC-Pad4)"
      },
      {
        "netclass": "Default",
        "pattern": "Net-(U16-SW)"
      },
      {
        "netclass": "Default",
        "pattern": "Net-(Q3-B)"
      },
      {
        "netclass": "Default",
        "pattern": "/CM4_HighSpeed/PCIE_CLK_P"
      },
      {
        "netclass": "Default",
        "pattern": "unconnected-(Module1A-Ethernet_nLED1(3.3v)-Pad19)"
      },
      {
        "netclass": "Default",
        "pattern": "Net-(C57-Pad1)"
      },
      {
        "netclass": "Default",
        "pattern": "unconnected-(U3-VC1-Pad11)"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/d_dir"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/breakout/b_dir"
      },
      {
        "netclass": "Default",
        "pattern": "Net-(J7-DET_B)"
      },
      {
        "netclass": "Default",
        "pattern": "unconnected-(Module1A-SD_DAT6-Pad72)"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/d_home+"
      },
      {
        "netclass": "Default",
        "pattern": "Net-(D8-A)"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/breakout/b_step_iso"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/breakout/fltc"
      },
      {
        "netclass": "Default",
        "pattern": "/CM4_GPIO ( Ethernet, GPIO, SDCARD)/GPIO9"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/breakout/c_dir_iso"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/breakout/stepper_enable"
      },
      {
        "netclass": "Default",
        "pattern": "Net-(J6-Pin_5)"
      },
      {
        "netclass": "Default",
        "pattern": "Net-(J6-Pin_4)"
      },
      {
        "netclass": "Default",
        "pattern": "/CM4_GPIO ( Ethernet, GPIO, SDCARD)/BT_nDis"
      },
      {
        "netclass": "Default",
        "pattern": "Net-(J4-Pin_5)"
      },
      {
        "netclass": "Default",
        "pattern": "Net-(U16-BST)"
      },
      {
        "netclass": "Default",
        "pattern": "/CM4_GPIO ( Ethernet, GPIO, SDCARD)/GPIO23"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/b_home-"
      },
      {
        "netclass": "Default",
        "pattern": "unconnected-(U8-NC-Pad4)"
      },
      {
        "netclass": "Default",
        "pattern": "/CM4_GPIO ( Ethernet, GPIO, SDCARD)/GPIO16"
      },
      {
        "netclass": "Default",
        "pattern": "/RTC , Wakeup, FAN/SCL"
      },
      {
        "netclass": "Default",
        "pattern": "/CM4_GPIO ( Ethernet, GPIO, SDCARD)/ETH_LEDY"
      },
      {
        "netclass": "Default",
        "pattern": "/CM4_GPIO ( Ethernet, GPIO, SDCARD)/GPIO18"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/breakout/e_dir_iso"
      },
      {
        "netclass": "Default",
        "pattern": "/CM4_GPIO ( Ethernet, GPIO, SDCARD)/GPIO4"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/breakout/flta"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/e_home-"
      },
      {
        "netclass": "Default",
        "pattern": "/CM4_GPIO ( Ethernet, GPIO, SDCARD)/GPIO19"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/breakout/e_step_iso"
      },
      {
        "netclass": "Default",
        "pattern": "/CM4_HighSpeed/PCIE_TX_P"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/a_step"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/breakout/c_step"
      },
      {
        "netclass": "Default",
        "pattern": "Net-(U21-VREF)"
      },
      {
        "netclass": "Default",
        "pattern": "Net-(J2-Pin_5)"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/b_step"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/breakout/d_home+"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/breakout/c_dir"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/+1V2"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/breakout/d_dir_iso"
      },
      {
        "netclass": "Default",
        "pattern": "Net-(D23-A)"
      },
      {
        "netclass": "Default",
        "pattern": "/CM4_GPIO ( Ethernet, GPIO, SDCARD)/GPIO22"
      },
      {
        "netclass": "Default",
        "pattern": "GND1"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/breakout/iout"
      },
      {
        "netclass": "Default",
        "pattern": "/CM4_HighSpeed/PCIE_CLK_nREQ"
      },
      {
        "netclass": "Default",
        "pattern": "unconnected-(D13-NC-Pad2)"
      },
      {
        "netclass": "Default",
        "pattern": "Net-(U4-D1+)"
      },
      {
        "netclass": "Default",
        "pattern": "/CM4_HighSpeed/HDMI1_HOTPLUG"
      },
      {
        "netclass": "Default",
        "pattern": "/CM4_HighSpeed/HDMI0_HOTPLUG"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/c_dir"
      },
      {
        "netclass": "Default",
        "pattern": "unconnected-(U12-NC-Pad4)"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/probe"
      },
      {
        "netclass": "Default",
        "pattern": "Net-(Q2-B)"
      },
      {
        "netclass": "Default",
        "pattern": "Net-(U16-COMP)"
      },
      {
        "netclass": "Default",
        "pattern": "/CM4_HighSpeed/HDMI1_SCL"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/+3V3_GND2"
      },
      {
        "netclass": "Default",
        "pattern": "/CM4_HighSpeed/TV_OUT"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/breakout/fault"
      },
      {
        "netclass": "Default",
        "pattern": "Net-(D6-A)"
      },
      {
        "netclass": "Default",
        "pattern": "/CM4_GPIO ( Ethernet, GPIO, SDCARD)/Reserved"
      },
      {
        "netclass": "Default",
        "pattern": "/CM4_GPIO ( Ethernet, GPIO, SDCARD)/GPIO25"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/breakout/fltd"
      },
      {
        "netclass": "Default",
        "pattern": "/CM4_GPIO ( Ethernet, GPIO, SDCARD)/ID_SD"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/d_home-"
      },
      {
        "netclass": "Default",
        "pattern": "/CM4_GPIO ( Ethernet, GPIO, SDCARD)/SD_PWR_ON"
      },
      {
        "netclass": "Default",
        "pattern": "/USB2-HUB/VBUS"
      },
      {
        "netclass": "Default",
        "pattern": "unconnected-(Module1A-SD_VDD_Override-Pad73)"
      },
      {
        "netclass": "Default",
        "pattern": "Net-(Q2-E)"
      },
      {
        "netclass": "Default",
        "pattern": "/CM4_HighSpeed/PCIE_CLK_N"
      },
      {
        "netclass": "Default",
        "pattern": "/CM4_HighSpeed/PCIE_RX_P"
      },
      {
        "netclass": "Default",
        "pattern": "/CM4_GPIO ( Ethernet, GPIO, SDCARD)/GPIO7"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/breakout/spindle_pwm_iso"
      },
      {
        "netclass": "Default",
        "pattern": "GND2"
      },
      {
        "netclass": "Default",
        "pattern": "Net-(Q1-D)"
      },
      {
        "netclass": "Default",
        "pattern": "/CM4_GPIO ( Ethernet, GPIO, SDCARD)/GPIO24"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/a_home-"
      },
      {
        "netclass": "Default",
        "pattern": "/nEXTRST"
      },
      {
        "netclass": "Default",
        "pattern": "/CM4_HighSpeed/HDMI0_SCL"
      },
      {
        "netclass": "Default",
        "pattern": "unconnected-(D5-NC-Pad2)"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/pwm1"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/VCCPLL_1V2"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/breakout/a_dir_iso"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/breakout/spindle_rev_iso"
      },
      {
        "netclass": "Default",
        "pattern": "/CM4_HighSpeed/HDMI1_CEC"
      },
      {
        "netclass": "Default",
        "pattern": "unconnected-(U11-nALERT-Pad8)"
      },
      {
        "netclass": "Default",
        "pattern": "unconnected-(U20-IND-Pad11)"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/breakout/fltb"
      },
      {
        "netclass": "Default",
        "pattern": "/CM4_GPIO ( Ethernet, GPIO, SDCARD)/GPIO20"
      },
      {
        "netclass": "Default",
        "pattern": "Net-(R10-Pad2)"
      },
      {
        "netclass": "Default",
        "pattern": "/CM4_GPIO ( Ethernet, GPIO, SDCARD)/nPWR_LED"
      },
      {
        "netclass": "Default",
        "pattern": "/CM4_GPIO ( Ethernet, GPIO, SDCARD)/SD_CLK"
      },
      {
        "netclass": "Default",
        "pattern": "/USB2-HUB/nOCS1"
      },
      {
        "netclass": "Default",
        "pattern": "/CM4_GPIO ( Ethernet, GPIO, SDCARD)/EEPROM_nWP"
      },
      {
        "netclass": "Default",
        "pattern": "/CM4_GPIO ( Ethernet, GPIO, SDCARD)/GPIO14"
      },
      {
        "netclass": "Default",
        "pattern": "/CM4_HighSpeed/PCIE_RX_N"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/c_step"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/clk_8mhz"
      },
      {
        "netclass": "Default",
        "pattern": "/CM4_GPIO ( Ethernet, GPIO, SDCARD)/CAM_GPIO"
      },
      {
        "netclass": "Default",
        "pattern": "Net-(J5-Pin_5)"
      },
      {
        "netclass": "Default",
        "pattern": "/USB2-HUB/PWR1"
      },
      {
        "netclass": "Default",
        "pattern": "Net-(X1-OUT)"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/breakout/+5V_ISO"
      },
      {
        "netclass": "Default",
        "pattern": "Net-(J3-Pin_5)"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/breakout/b_step"
      },
      {
        "netclass": "Default",
        "pattern": "/CM4_GPIO ( Ethernet, GPIO, SDCARD)/ETH_LEDG"
      },
      {
        "netclass": "Default",
        "pattern": "Net-(C62-Pad1)"
      },
      {
        "netclass": "Default",
        "pattern": "unconnected-(U6B-IOB_29b-Pad19)"
      },
      {
        "netclass": "Default",
        "pattern": "GND"
      },
      {
        "netclass": "Default",
        "pattern": "/CM4_GPIO ( Ethernet, GPIO, SDCARD)/GPIO5"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/e_home+"
      },
      {
        "netclass": "Default",
        "pattern": "unconnected-(D9-NC-Pad2)"
      },
      {
        "netclass": "Default",
        "pattern": "/CM4_GPIO ( Ethernet, GPIO, SDCARD)/nRPIBOOT"
      },
      {
        "netclass": "Default",
        "pattern": "/CM4_GPIO ( Ethernet, GPIO, SDCARD)/GPIO15"
      },
      {
        "netclass": "Default",
        "pattern": "/CM4_GPIO ( Ethernet, GPIO, SDCARD)/SD_DAT1"
      },
      {
        "netclass": "Default",
        "pattern": "Net-(U4-D1-)"
      },
      {
        "netclass": "Default",
        "pattern": "Net-(U16-SS)"
      },
      {
        "netclass": "Default",
        "pattern": "Net-(D3-A)"
      },
      {
        "netclass": "Default",
        "pattern": "unconnected-(U18-nFLG-Pad3)"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/breakout/e_dir"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/breakout/spindle_fwd"
      },
      {
        "netclass": "Default",
        "pattern": "Net-(J2-Pin_4)"
      },
      {
        "netclass": "Default",
        "pattern": "Net-(J8-Pin_1)"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/breakout/e_home+"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/breakout/e_step"
      },
      {
        "netclass": "Default",
        "pattern": "unconnected-(U6B-IOB_31b-Pad18)"
      },
      {
        "netclass": "Default",
        "pattern": "Net-(U7-ILIM)"
      },
      {
        "netclass": "Default",
        "pattern": "/CM4_GPIO ( Ethernet, GPIO, SDCARD)/SD_DAT2"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/breakout/a_step_iso"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/breakout/c_step_iso"
      },
      {
        "netclass": "Default",
        "pattern": "Net-(Q4-B)"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/a_dir"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/b_dir"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/breakout/spindle_fwd_oc"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/c_home+"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/stepper_enable"
      },
      {
        "netclass": "Default",
        "pattern": "Net-(D21-A)"
      },
      {
        "netclass": "Default",
        "pattern": "Net-(D16-A)"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/breakout/c_home+"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/spindle_rev"
      },
      {
        "netclass": "Default",
        "pattern": "Net-(D4-A)"
      },
      {
        "netclass": "Default",
        "pattern": "Net-(J17-Pin_4)"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/c_home-"
      },
      {
        "netclass": "Default",
        "pattern": "unconnected-(Module1B-Reserved-Pad106)"
      },
      {
        "netclass": "Default",
        "pattern": "unconnected-(U3-VC3-Pad13)"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/breakout/flte"
      },
      {
        "netclass": "Default",
        "pattern": "Net-(J5-Pin_4)"
      },
      {
        "netclass": "Default",
        "pattern": "Net-(J7-DET_A)"
      },
      {
        "netclass": "Default",
        "pattern": "/CM4_GPIO ( Ethernet, GPIO, SDCARD)/GPIO17"
      },
      {
        "netclass": "Default",
        "pattern": "unconnected-(Module1A-SD_DAT4-Pad68)"
      },
      {
        "netclass": "Default",
        "pattern": "/CM4_GPIO ( Ethernet, GPIO, SDCARD)/SD_DAT0"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/d_step"
      },
      {
        "netclass": "Default",
        "pattern": "unconnected-(Module1A-SD_DAT5-Pad64)"
      },
      {
        "netclass": "Default",
        "pattern": "/CM4_HighSpeed/PCIE_nRST"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/breakout/a_step"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/breakout/e_home-"
      },
      {
        "netclass": "Default",
        "pattern": "Net-(D2-K)"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/breakout/spindle_pwm"
      },
      {
        "netclass": "Default",
        "pattern": "/CM4_GPIO ( Ethernet, GPIO, SDCARD)/GPIO11"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/breakout/a_dir"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/breakout/estop"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/breakout/d_dir"
      },
      {
        "netclass": "Default",
        "pattern": "unconnected-(U11-CLK-Pad7)"
      },
      {
        "netclass": "Default",
        "pattern": "unconnected-(U6A-RGB0-Pad39)"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/pwm0"
      },
      {
        "netclass": "Default",
        "pattern": "Net-(U3-LEDG_K)"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/breakout/a_home-"
      },
      {
        "netclass": "Default",
        "pattern": "Net-(D1-K)"
      },
      {
        "netclass": "Default",
        "pattern": "Net-(J4-Pin_4)"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/e_step"
      },
      {
        "netclass": "Default",
        "pattern": "/CM4_GPIO ( Ethernet, GPIO, SDCARD)/AIN0"
      },
      {
        "netclass": "Default",
        "pattern": "/CM4_HighSpeed/PCIE_TX_N"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/spindle_fwd"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/breakout/fault_iso"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/breakout/a_home+"
      },
      {
        "netclass": "Default",
        "pattern": "/CM4_GPIO ( Ethernet, GPIO, SDCARD)/GPIO27"
      },
      {
        "netclass": "Default",
        "pattern": "GND3"
      },
      {
        "netclass": "Default",
        "pattern": "Net-(C1-Pad1)"
      },
      {
        "netclass": "Default",
        "pattern": "Net-(D15-A)"
      },
      {
        "netclass": "Default",
        "pattern": "Net-(U21-IIN)"
      },
      {
        "netclass": "Default",
        "pattern": "/CM4_HighSpeed/HDMI0_CEC"
      },
      {
        "netclass": "Default",
        "pattern": "Net-(U3-LEDY_K)"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/+5V_GND2"
      },
      {
        "netclass": "Default",
        "pattern": "Net-(D18-A)"
      },
      {
        "netclass": "Default",
        "pattern": "unconnected-(U6B-IOB_18a-Pad10)"
      },
      {
        "netclass": "Default",
        "pattern": "Net-(D12-A)"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/breakout/+VS"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/breakout/spindle_rev"
      },
      {
        "netclass": "Default",
        "pattern": "unconnected-(Module1A-SD_DAT7-Pad70)"
      },
      {
        "netclass": "Default",
        "pattern": "/+5v"
      },
      {
        "netclass": "Default",
        "pattern": "/CM4_GPIO ( Ethernet, GPIO, SDCARD)/GPIO21"
      },
      {
        "netclass": "Default",
        "pattern": "unconnected-(D7-NC-Pad2)"
      },
      {
        "netclass": "Default",
        "pattern": "Net-(Module1A-PI_nLED_Activity)"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/breakout/c_home-"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/breakout/spindle_fwd_iso"
      },
      {
        "netclass": "Default",
        "pattern": "/CM4_GPIO ( Ethernet, GPIO, SDCARD)/+1.8v"
      },
      {
        "netclass": "Default",
        "pattern": "/CM4_GPIO ( Ethernet, GPIO, SDCARD)/GPIO2"
      },
      {
        "netclass": "Default",
        "pattern": "/CM4_GPIO ( Ethernet, GPIO, SDCARD)/GPIO8"
      },
      {
        "netclass": "Default",
        "pattern": "unconnected-(U20-OUTD-Pad6)"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/breakout/b_dir_iso"
      },
      {
        "netclass": "Default",
        "pattern": "Net-(D14-A)"
      },
      {
        "netclass": "Default",
        "pattern": "/CM4_GPIO ( Ethernet, GPIO, SDCARD)/GPIO6"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/e_dir"
      },
      {
        "netclass": "Default",
        "pattern": "/CM4_GPIO ( Ethernet, GPIO, SDCARD)/SD_DAT3"
      },
      {
        "netclass": "Default",
        "pattern": "/CM4_GPIO ( Ethernet, GPIO, SDCARD)/SD_CMD"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/breakout/probe"
      },
      {
        "netclass": "Default",
        "pattern": "/CM4_GPIO ( Ethernet, GPIO, SDCARD)/GPIO26"
      },
      {
        "netclass": "Default",
        "pattern": "unconnected-(X1-Tri-State-Pad1)"
      },
      {
        "netclass": "Default",
        "pattern": "/CM4_GPIO ( Ethernet, GPIO, SDCARD)/SYNC_OUT"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/breakout/d_home-"
      },
      {
        "netclass": "Default",
        "pattern": "/CM4_GPIO ( Ethernet, GPIO, SDCARD)/GPIO13"
      },
      {
        "netclass": "Default",
        "pattern": "/CM4_GPIO ( Ethernet, GPIO, SDCARD)/SD_PWR"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/breakout/d_step"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/breakout/spindle_rev_oc"
      },
      {
        "netclass": "Default",
        "pattern": "unconnected-(Module1B-Reserved-Pad104)"
      },
      {
        "netclass": "Default",
        "pattern": "unconnected-(U6A-RGB2-Pad41)"
      },
      {
        "netclass": "Default",
        "pattern": "/CM4_GPIO ( Ethernet, GPIO, SDCARD)/ID_SC"
      },
      {
        "netclass": "Default",
        "pattern": "unconnected-(U3-VC4-Pad14)"
      },
      {
        "netclass": "Default",
        "pattern": "/CM4_GPIO ( Ethernet, GPIO, SDCARD)/GPIO10"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/breakout/b_home-"
      },
      {
        "netclass": "Default",
        "pattern": "Net-(J3-Pin_4)"
      },
      {
        "netclass": "Default",
        "pattern": "Net-(D10-A)"
      },
      {
        "netclass": "Default",
        "pattern": "Net-(J8-Pin_2)"
      },
      {
        "netclass": "Default",
        "pattern": "/CM4_GPIO ( Ethernet, GPIO, SDCARD)/SYNC_IN"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/b_home+"
      },
      {
        "netclass": "Default",
        "pattern": "Net-(C56-Pad1)"
      },
      {
        "netclass": "Default",
        "pattern": "Net-(J17-Pin_3)"
      },
      {
        "netclass": "Default",
        "pattern": "/FPGA/breakout/b_home+"
      },
      {
        "netclass": "Default",
        "pattern": "Net-(U16-FB)"
      },
      {
        "netclass": "Default",
        "pattern": "Net-(D19-A)"
      },
      {
        "netclass": "Default",
        "pattern": "Net-(D22-A)"
      },
      {
        "netclass": "Default",
        "pattern": "Net-(C60-Pad1)"
      },
      {
        "netclass": "Default",
        "pattern": "/CM4_HighSpeed/HDMI1_SDA"
      },
      {
        "netclass": "Default",
        "pattern": "/CM4_GPIO ( Ethernet, GPIO, SDCARD)/WL_nDis"
      },
      {
        "netclass": "Default",
        "pattern": "Net-(J8-Pin_3)"
      },
      {
        "netclass": "100R",
        "pattern": "/CM4_GPIO ( Ethernet, GPIO, SDCARD)/TRD0_N"
      },
      {
        "netclass": "100R",
        "pattern": "/CM4_GPIO ( Ethernet, GPIO, SDCARD)/TRD0_P"
      },
      {
        "netclass": "100R",
        "pattern": "/CM4_GPIO ( Ethernet, GPIO, SDCARD)/TRD1_N"
      },
      {
        "netclass": "100R",
        "pattern": "/CM4_GPIO ( Ethernet, GPIO, SDCARD)/TRD1_P"
      },
      {
        "netclass": "100R",
        "pattern": "/CM4_GPIO ( Ethernet, GPIO, SDCARD)/TRD2_N"
      },
      {
        "netclass": "100R",
        "pattern": "/CM4_GPIO ( Ethernet, GPIO, SDCARD)/TRD2_P"
      },
      {
        "netclass": "100R",
        "pattern": "/CM4_GPIO ( Ethernet, GPIO, SDCARD)/TRD3_N"
      },
      {
        "netclass": "100R",
        "pattern": "/CM4_GPIO ( Ethernet, GPIO, SDCARD)/TRD3_P"
      },
      {
        "netclass": "100R",
        "pattern": "/CM4_HighSpeed/CAM0_C_N"
      },
      {
        "netclass": "100R",
        "pattern": "/CM4_HighSpeed/CAM0_C_P"
      },
      {
        "netclass": "100R",
        "pattern": "/CM4_HighSpeed/CAM0_D0_N"
      },
      {
        "netclass": "100R",
        "pattern": "/CM4_HighSpeed/CAM0_D0_P"
      },
      {
        "netclass": "100R",
        "pattern": "/CM4_HighSpeed/CAM0_D1_N"
      },
      {
        "netclass": "100R",
        "pattern": "/CM4_HighSpeed/CAM0_D1_P"
      },
      {
        "netclass": "100R",
        "pattern": "/CM4_HighSpeed/CAM1_C_N"
      },
      {
        "netclass": "100R",
        "pattern": "/CM4_HighSpeed/CAM1_C_P"
      },
      {
        "netclass": "100R",
        "pattern": "/CM4_HighSpeed/CAM1_D0_N"
      },
      {
        "netclass": "100R",
        "pattern": "/CM4_HighSpeed/CAM1_D0_P"
      },
      {
        "netclass": "100R",
        "pattern": "/CM4_HighSpeed/CAM1_D1_N"
      },
      {
        "netclass": "100R",
        "pattern": "/CM4_HighSpeed/CAM1_D1_P"
      },
      {
        "netclass": "100R",
        "pattern": "/CM4_HighSpeed/CAM1_D2_N"
      },
      {
        "netclass": "100R",
        "pattern": "/CM4_HighSpeed/CAM1_D2_P"
      },
      {
        "netclass": "100R",
        "pattern": "/CM4_HighSpeed/CAM1_D3_N"
      },
      {
        "netclass": "100R",
        "pattern": "/CM4_HighSpeed/CAM1_D3_P"
      },
      {
        "netclass": "100R",
        "pattern": "/CM4_HighSpeed/DSI0_C_N"
      },
      {
        "netclass": "100R",
        "pattern": "/CM4_HighSpeed/DSI0_C_P"
      },
      {
        "netclass": "100R",
        "pattern": "/CM4_HighSpeed/DSI0_D0_N"
      },
      {
        "netclass": "100R",
        "pattern": "/CM4_HighSpeed/DSI0_D0_P"
      },
      {
        "netclass": "100R",
        "pattern": "/CM4_HighSpeed/DSI0_D1_N"
      },
      {
        "netclass": "100R",
        "pattern": "/CM4_HighSpeed/DSI0_D1_P"
      },
      {
        "netclass": "100R",
        "pattern": "/CM4_HighSpeed/DSI1_C_N"
      },
      {
        "netclass": "100R",
        "pattern": "/CM4_HighSpeed/DSI1_C_P"
      },
      {
        "netclass": "100R",
        "pattern": "/CM4_HighSpeed/DSI1_D0_N"
      },
      {
        "netclass": "100R",
        "pattern": "/CM4_HighSpeed/DSI1_D0_P"
      },
      {
        "netclass": "100R",
        "pattern": "/CM4_HighSpeed/DSI1_D1_N"
      },
      {
        "netclass": "100R",
        "pattern": "/CM4_HighSpeed/DSI1_D1_P"
      },
      {
        "netclass": "100R",
        "pattern": "/CM4_HighSpeed/DSI1_D2_N"
      },
      {
        "netclass": "100R",
        "pattern": "/CM4_HighSpeed/DSI1_D2_P"
      },
      {
        "netclass": "100R",
        "pattern": "/CM4_HighSpeed/DSI1_D3_N"
      },
      {
        "netclass": "100R",
        "pattern": "/CM4_HighSpeed/DSI1_D3_P"
      },
      {
        "netclass": "90R",
        "pattern": "/USB2-HUB/HD1_N"
      },
      {
        "netclass": "90R",
        "pattern": "/USB2-HUB/HD1_P"
      },
      {
        "netclass": "90R",
        "pattern": "/USB2-HUB/HD2_N"
      },
      {
        "netclass": "90R",
        "pattern": "/USB2-HUB/HD2_P"
      },
      {
        "netclass": "90R",
        "pattern": "/USB2-HUB/HD3_N"
      },
      {
        "netclass": "90R",
        "pattern": "/USB2-HUB/HD3_P"
      },
      {
        "netclass": "90R",
        "pattern": "/USB2-HUB/HD4_N"
      },
      {
        "netclass": "90R",
        "pattern": "/USB2-HUB/HD4_P"
      },
      {
        "netclass": "90R",
        "pattern": "/USB2-HUB/USBD_N"
      },
      {
        "netclass": "90R",
        "pattern": "/USB2-HUB/USBD_P"
      },
      {
        "netclass": "90R",
        "pattern": "/USB2-HUB/USBH_N"
      },
      {
        "netclass": "90R",
        "pattern": "/USB2-HUB/USBH_P"
      },
      {
        "netclass": "HDMI",
        "pattern": "/CM4_HighSpeed/HDMI0_CK_N"
      },
      {
        "netclass": "HDMI",
        "pattern": "/CM4_HighSpeed/HDMI0_CK_P"
      },
      {
        "netclass": "HDMI",
        "pattern": "/CM4_HighSpeed/HDMI0_D0_N"
      },
      {
        "netclass": "HDMI",
        "pattern": "/CM4_HighSpeed/HDMI0_D0_P"
      },
      {
        "netclass": "HDMI",
        "pattern": "/CM4_HighSpeed/HDMI0_D1_N"
      },
      {
        "netclass": "HDMI",
        "pattern": "/CM4_HighSpeed/HDMI0_D1_P"
      },
      {
        "netclass": "HDMI",
        "pattern": "/CM4_HighSpeed/HDMI0_D2_N"
      },
      {
        "netclass": "HDMI",
        "pattern": "/CM4_HighSpeed/HDMI0_D2_P"
      },
      {
        "netclass": "HDMI",
        "pattern": "/CM4_HighSpeed/HDMI1_CK_N"
      },
      {
        "netclass": "HDMI",
        "pattern": "/CM4_HighSpeed/HDMI1_CK_P"
      },
      {
        "netclass": "HDMI",
        "pattern": "/CM4_HighSpeed/HDMI1_D0_N"
      },
      {
        "netclass": "HDMI",
        "pattern": "/CM4_HighSpeed/HDMI1_D0_P"
      },
      {
        "netclass": "HDMI",
        "pattern": "/CM4_HighSpeed/HDMI1_D1_N"
      },
      {
        "netclass": "HDMI",
        "pattern": "/CM4_HighSpeed/HDMI1_D1_P"
      },
      {
        "netclass": "HDMI",
        "pattern": "/CM4_HighSpeed/HDMI1_D2_N"
      },
      {
        "netclass": "HDMI",
        "pattern": "/CM4_HighSpeed/HDMI1_D2_P"
      },
      {
        "netclass": "POE TAPS",
        "pattern": "/CM4_GPIO ( Ethernet, GPIO, SDCARD)/TR0_TAP"
      },
      {
        "netclass": "POE TAPS",
        "pattern": "/CM4_GPIO ( Ethernet, GPIO, SDCARD)/TR1_TAP"
      },
      {
        "netclass": "POE TAPS",
        "pattern": "/CM4_GPIO ( Ethernet, GPIO, SDCARD)/TR2_TAP"
      },
      {
        "netclass": "POE TAPS",
        "pattern": "/CM4_GPIO ( Ethernet, GPIO, SDCARD)/TR3_TAP"
      }
    ]
  },
  "pcbnew": {
    "last_paths": {
      "gencad": "",
      "idf": "",
      "netlist": "",
      "plot": "",
      "pos_files": "",
      "specctra_dsn": "",
      "step": "",
      "svg": "",
      "vrml": ""
    },
    "page_layout_descr_file": ""
  },
  "schematic": {
    "legacy_lib_dir": "",
    "legacy_lib_list": []
  },
  "sheets": [],
  "text_variables": {}
}