(module "BarrelJack_Horizontal" (layer F.Cu) (tedit 5EF86901)
  (descr "DC Barrel Jack")
  (tags "Power Jack")
  (fp_text reference "J19" (at 2.425 -3.95 90) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value "Barrel_Jack" (at -6.2 -5.5) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user "${REFERENCE}" (at -3 -2.95) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -0.003213 -4.505425) (end 0.8 -3.75) (layer F.Fab) (width 0.1))
  (fp_line (start 1.1 -3.75) (end 1.1 -4.8) (layer F.SilkS) (width 0.12))
  (fp_line (start 0.05 -4.8) (end 1.1 -4.8) (layer F.SilkS) (width 0.12))
  (fp_line (start 1 -4.5) (end 1 -4.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1 -4.75) (end -14 -4.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1 -4.5) (end 1 -2) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1 -2) (end 2 -2) (layer F.CrtYd) (width 0.05))
  (fp_line (start 2 -2) (end 2 2) (layer F.CrtYd) (width 0.05))
  (fp_line (start 2 2) (end 1 2) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1 2) (end 1 4.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1 4.75) (end -1 4.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1 4.75) (end -1 6.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1 6.75) (end -5 6.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start -5 6.75) (end -5 4.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start -5 4.75) (end -14 4.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start -14 4.75) (end -14 -4.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start -5.9 4.6) (end -13.8 4.6) (layer F.SilkS) (width 0.12))
  (fp_line (start -13.8 4.6) (end -13.8 -4.6) (layer F.SilkS) (width 0.12))
  (fp_line (start 0.9 2.7) (end 0.9 4.6) (layer F.SilkS) (width 0.12))
  (fp_line (start 0.9 4.6) (end -0.1 4.6) (layer F.SilkS) (width 0.12))
  (fp_line (start -13.8 -4.6) (end 0.9 -4.6) (layer F.SilkS) (width 0.12))
  (fp_line (start 0.9 -4.6) (end 0.9 -2.6) (layer F.SilkS) (width 0.12))
  (fp_line (start -10.2 -4.5) (end -10.2 4.5) (layer F.Fab) (width 0.1))
  (fp_line (start -13.7 -4.5) (end -13.7 4.5) (layer F.Fab) (width 0.1))
  (fp_line (start -13.7 4.5) (end 0.8 4.5) (layer F.Fab) (width 0.1))
  (fp_line (start 0.8 4.5) (end 0.8 -3.75) (layer F.Fab) (width 0.1))
  (fp_line (start 0 -4.5) (end -13.7 -4.5) (layer F.Fab) (width 0.1))
  (pad "1" thru_hole oval (at 0 0) (size 2.8 5) (drill oval 0.8 3) (layers *.Cu *.Mask) (tstamp 980d9fb0-1967-4ebe-8791-f3420d870ffe))
  (pad "2" thru_hole roundrect (at -5.8 0) (size 2.8 5) (drill oval 0.8 3) (layers *.Cu *.Mask) (roundrect_rratio 0.25) (tstamp 2c5611bf-1068-4220-8774-4234768f031d))
  (pad "3" thru_hole roundrect (at -3 4.8) (size 5 2.8) (drill oval 3 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25) (tstamp be6da788-4b46-48f8-93d4-2cf95c79c0f6))
  (model "./CM4IO.3dshapes/CUI_DEVICES_PJ-102AH.step"
    (offset (xyz -13.7 0 6.5))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 180))
  )
)
