(module Analog_CP-24-14 (layer F.Cu) (tedit 5D819C21)
  (fp_text reference REF** (at 0 0) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value %R (at 0 -0.5) (layer F.Fab) hide
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user %R (at 0 0) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -2.2 -1.625) (end -1.625 -2.2) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.2 2.2) (end -2.2 1.625) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.625 2.2) (end -2.2 2.2) (layer F.SilkS) (width 0.15))
  (fp_line (start 1.625 2.2) (end 2.2 2.2) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.2 2.2) (end 2.2 1.625) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.2 -1.625) (end 2.2 -2.2) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.2 -2.2) (end 1.625 -2.2) (layer F.SilkS) (width 0.15))
  (fp_circle (center -2.2 -2.2) (end -2.2 -2.35) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.75 -2.05) (end -2.05 -1.75) (layer F.Fab) (width 0.15))
  (fp_line (start 2.05 -2.05) (end -1.75 -2.05) (layer F.Fab) (width 0.15))
  (fp_line (start 2.05 2.05) (end 2.05 -2.05) (layer F.Fab) (width 0.15))
  (fp_line (start -2.05 2.05) (end 2.05 2.05) (layer F.Fab) (width 0.15))
  (fp_line (start -2.05 -1.75) (end -2.05 2.05) (layer F.Fab) (width 0.15))
  (fp_line (start -2.3 -1.525) (end -2.3 -2.3) (layer F.CrtYd) (width 0.15))
  (fp_line (start -2.3 -2.3) (end 2.3 -2.3) (layer F.CrtYd) (width 0.15))
  (fp_line (start 2.3 -2.3) (end 2.3 -1.525) (layer F.CrtYd) (width 0.15))
  (fp_line (start 2.3 -1.525) (end 2.2 -1.525) (layer F.CrtYd) (width 0.15))
  (fp_line (start 2.2 -1.525) (end 2.2 1.525) (layer F.CrtYd) (width 0.15))
  (fp_line (start 2.2 1.525) (end 2.3 1.525) (layer F.CrtYd) (width 0.15))
  (fp_line (start 2.3 1.525) (end 2.3 2.3) (layer F.CrtYd) (width 0.15))
  (fp_line (start 2.3 2.3) (end -2.3 2.3) (layer F.CrtYd) (width 0.15))
  (fp_line (start -2.3 2.3) (end -2.3 1.525) (layer F.CrtYd) (width 0.15))
  (fp_line (start -2.3 1.525) (end -2.2 1.525) (layer F.CrtYd) (width 0.15))
  (fp_line (start -2.2 1.525) (end -2.2 -1.525) (layer F.CrtYd) (width 0.15))
  (fp_line (start -2.2 -1.525) (end -2.3 -1.525) (layer F.CrtYd) (width 0.15))
  (pad 1 smd rect (at -1.8 -1.25) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.05))
  (pad 2 smd rect (at -1.8 -0.75) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.05))
  (pad 3 smd rect (at -1.8 -0.25) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.05))
  (pad 4 smd rect (at -1.8 0.25) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.05))
  (pad 5 smd rect (at -1.8 0.75) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.05))
  (pad 6 smd rect (at -1.8 1.25) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.05))
  (pad 7 smd rect (at -1.25 1.8) (size 0.35 0.5) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.05))
  (pad 8 smd rect (at -0.75 1.8) (size 0.35 0.5) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.05))
  (pad 9 smd rect (at -0.25 1.8) (size 0.35 0.5) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.05))
  (pad 10 smd rect (at 0.25 1.8) (size 0.35 0.5) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.05))
  (pad 11 smd rect (at 0.75 1.8) (size 0.35 0.5) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.05))
  (pad 12 smd rect (at 1.25 1.8) (size 0.35 0.5) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.05))
  (pad 13 smd rect (at 1.8 1.25) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.05))
  (pad 14 smd rect (at 1.8 0.75) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.05))
  (pad 15 smd rect (at 1.8 0.25) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.05))
  (pad 16 smd rect (at 1.8 -0.25) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.05))
  (pad 17 smd rect (at 1.8 -0.75) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.05))
  (pad 18 smd rect (at 1.8 -1.25) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.05))
  (pad 19 smd rect (at 1.25 -1.8) (size 0.35 0.5) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.05))
  (pad 20 smd rect (at 0.75 -1.8) (size 0.35 0.5) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.05))
  (pad 21 smd rect (at 0.25 -1.8) (size 0.35 0.5) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.05))
  (pad 22 smd rect (at -0.25 -1.8) (size 0.35 0.5) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.05))
  (pad 23 smd rect (at -0.75 -1.8) (size 0.35 0.5) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.05))
  (pad 24 smd rect (at -1.25 -1.8) (size 0.35 0.5) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.05))
  (pad 0 smd rect (at 0 0) (size 2.44 2.44) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.05))
)
