(module Analog-DFN8-EP (layer F.Cu) (tedit 5D819C58)
  (fp_text reference REF** (at 0.0 0.0) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user %R (at 0.0 0.0) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value %V (at 0 -0.5) (layer F.Fab) hide
    (effects (font (size 1 1) (thickness 0.15)))
  )

  (fp_line (start -1.7 -1.1) (end -1.1 -1.7) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.1 -1.7) (end 1.7 -1.7) (layer F.SilkS) (width 0.15))
  (fp_line (start 1.7 -1.7) (end 1.7 -1.1) (layer F.SilkS) (width 0.15))
  (fp_line (start 1.7 1.1) (end 1.7 1.7) (layer F.SilkS) (width 0.15))
  (fp_line (start 1.7 1.7) (end -1.7 1.7) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.7 1.7) (end -1.7 1.1) (layer F.SilkS) (width 0.15))
  (fp_circle (center -1.4125 -2.0749999999999997) (end -1.4125 -1.9249999999999998) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.25 -1.55) (end -1.55 -1.25) (layer F.Fab) (width 0.15))
  (fp_line (start 1.55 -1.55) (end -1.25 -1.55) (layer F.Fab) (width 0.15))
  (fp_line (start 1.55 1.55) (end 1.55 -1.55) (layer F.Fab) (width 0.15))
  (fp_line (start -1.55 1.55) (end 1.55 1.55) (layer F.Fab) (width 0.15))
  (fp_line (start -1.55 -1.25) (end -1.55 1.55) (layer F.Fab) (width 0.15))
  (fp_line (start 1.875 -1.7) (end -1.875 -1.7) (layer F.CrtYd) (width 0.15))
  (fp_line (start -1.875 -1.7) (end -1.875 1.7) (layer F.CrtYd) (width 0.15))
  (fp_line (start -1.875 1.7) (end 1.875 1.7) (layer F.CrtYd) (width 0.15))
  (fp_line (start 1.875 1.7) (end 1.875 -1.7) (layer F.CrtYd) (width 0.15))
  (pad 1 smd rect (at -1.4125 -0.75) (size 0.7249999999999999 0.3) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.05))
  (pad 2 smd rect (at -1.4125 -0.25) (size 0.7249999999999999 0.3) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.05))
  (pad 3 smd rect (at -1.4125 0.25) (size 0.7249999999999999 0.3) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.05))
  (pad 4 smd rect (at -1.4125 0.75) (size 0.7249999999999999 0.3) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.05))
  (pad 5 smd rect (at 1.4125 0.75) (size 0.7249999999999999 0.3) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.05))
  (pad 6 smd rect (at 1.4125 0.25) (size 0.7249999999999999 0.3) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.05))
  (pad 7 smd rect (at 1.4125 -0.25) (size 0.7249999999999999 0.3) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.05))
  (pad 8 smd rect (at 1.4125 -0.75) (size 0.7249999999999999 0.3) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.05))
  (pad 0 smd rect (at 0 0) (size 1.7 2.43) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.05))
)
