(module ServoLayout (layer F.Cu) (tedit 5E952C68)
  (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value ServoLayout (at 0 -0.5) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -6.1 18.5) (end 6.1 18.5) (layer Cmts.User) (width 0.12))
  (fp_line (start 6.1 18.5) (end 6.1 41.5) (layer Cmts.User) (width 0.12))
  (fp_line (start 6.1 41.5) (end -6.1 41.5) (layer Cmts.User) (width 0.12))
  (fp_line (start -6.1 41.5) (end -6.1 18.5) (layer Cmts.User) (width 0.12))
  (fp_line (start 6.1 -41.5) (end 6.1 -18.5) (layer Cmts.User) (width 0.12))
  (fp_line (start -6.1 -41.5) (end 6.1 -41.5) (layer Cmts.User) (width 0.12))
  (fp_line (start 6.1 -18.5) (end -6.1 -18.5) (layer Cmts.User) (width 0.12))
  (fp_line (start -6.1 -18.5) (end -6.1 -41.5) (layer Cmts.User) (width 0.12))
  (fp_line (start 41.5 6.1) (end 18.5 6.1) (layer Cmts.User) (width 0.12))
  (fp_line (start 41.5 -6.1) (end 41.5 6.1) (layer Cmts.User) (width 0.12))
  (fp_line (start -18.5 6.1) (end -41.5 6.1) (layer Cmts.User) (width 0.12))
  (fp_line (start 18.5 6.1) (end 18.5 -6.1) (layer Cmts.User) (width 0.12))
  (fp_line (start 18.5 -6.1) (end 41.5 -6.1) (layer Cmts.User) (width 0.12))
  (fp_line (start -18.5 -6.1) (end -18.5 6.1) (layer Cmts.User) (width 0.12))
  (fp_line (start -41.5 6.1) (end -41.5 -6.1) (layer Cmts.User) (width 0.12))
  (fp_line (start -41.5 -6.1) (end -18.5 -6.1) (layer Cmts.User) (width 0.12))
  (fp_line (start -14 -6) (end -14 6) (layer Cmts.User) (width 0.12))
  (fp_line (start -14 6) (end -46 6) (layer Cmts.User) (width 0.12))
  (fp_line (start -46 6) (end -46 -6) (layer Cmts.User) (width 0.12))
  (fp_line (start -46 -6) (end -14 -6) (layer Cmts.User) (width 0.12))
  (fp_line (start 6 46) (end -6 46) (layer Cmts.User) (width 0.12))
  (fp_line (start -6 46) (end -6 14) (layer Cmts.User) (width 0.12))
  (fp_line (start -6 14) (end 6 14) (layer Cmts.User) (width 0.12))
  (fp_line (start 6 14) (end 6 46) (layer Cmts.User) (width 0.12))
  (fp_line (start 46 -6) (end 46 6) (layer Cmts.User) (width 0.12))
  (fp_line (start 46 6) (end 14 6) (layer Cmts.User) (width 0.12))
  (fp_line (start 14 6) (end 14 -6) (layer Cmts.User) (width 0.12))
  (fp_line (start 14 -6) (end 46 -6) (layer Cmts.User) (width 0.12))
  (fp_line (start -6 -46) (end 6 -46) (layer Cmts.User) (width 0.12))
  (fp_line (start 6 -46) (end 6 -14) (layer Cmts.User) (width 0.12))
  (fp_line (start 6 -14) (end -6 -14) (layer Cmts.User) (width 0.12))
  (fp_line (start -6 -14) (end -6 -46) (layer Cmts.User) (width 0.12))
  (pad "" np_thru_hole circle (at -16.15 0) (size 2 2) (drill 2) (layers *.Cu *.Paste *.Mask))
  (pad "" np_thru_hole circle (at -43.85 0) (size 2 2) (drill 2) (layers *.Cu *.Paste *.Mask)
    (solder_paste_margin 0.05))
  (pad "" np_thru_hole circle (at 0 16.15 90) (size 2 2) (drill 2) (layers *.Cu *.Paste *.Mask))
  (pad "" np_thru_hole circle (at 16.15 0 180) (size 2 2) (drill 2) (layers *.Cu *.Paste *.Mask))
  (pad "" np_thru_hole circle (at 0 -16.15 270) (size 2 2) (drill 2) (layers *.Cu *.Paste *.Mask))
  (pad "" np_thru_hole circle (at 0 43.85 90) (size 2 2) (drill 2) (layers *.Cu *.Paste *.Mask))
  (pad "" np_thru_hole circle (at 43.85 0 180) (size 2 2) (drill 2) (layers *.Cu *.Paste *.Mask)
    (solder_paste_margin 0.05))
  (pad "" np_thru_hole circle (at 0 -43.85 270) (size 2 2) (drill 2) (layers *.Cu *.Paste *.Mask)
    (solder_paste_margin 0.05))
)
